## The Project Gutenberg eBook of Implement sheds

This eBook is for the use of anyone anywhere in the United States and most other parts of the world at no cost and with almost no restrictions whatsoever. You may copy it, give it away or re-use it under the terms of the Project Gutenberg License included with this eBook or online at www.gutenberg.org. If you are not located in the United States, you will have to check the laws of the country where you are located before using this eBook.

Title: Implement sheds

Author: K. J. T. Ekblaw

Release date: April 2, 2016 [eBook #51639]
Most recently updated: October 23, 2024

Language: English

Other information and formats: www.gutenberg.org/ebooks/51639

Credits: Produced by Frank van Drogen, Harry Lamé and the Online
Distributed Proofreading Team at http://www.pgdp.net (This
file was produced from images generously made available
by The Internet Archive)

*** START OF THE PROJECT GUTENBERG EBOOK IMPLEMENT SHEDS ***

Copyright 1916
National Lumber Manufacturers Association

Over fifty million dollars is lost every year on American farms because implements and machinery are not properly housed. Is part of this wasted on YOUR farm?

Protection of farm machinery in well built implement sheds means dollars earned through dollars saved. On the average farm an implement shed saves annually as much as the income from $1,800 at interest.

# Implement Sheds

by
K. J. T. Ekblaw

Price, Ten Cents

Published by the
TRADE EXTENSION DEPARTMENT
National Lumber Manufacturers
Association
CHICAGO::ILLINOIS

APRIL, 1916

General Series No. 10

Fourth Edition, February, 1917.

Fig. 1. Exterior of Simple Implement Shed

Fig. 2. Perspective of Framing of Simple Implement Shed

Implement Sheds
By K. J. T. Ekblaw

A very fair indication of the thrift and general prosperity of a farmer is the method he employs in caring for his tools. Shiftlessness, waste, lack of energy, constant buying and heavy burdens of debt will accompany poor care. Good care is an indication of shrewdness, business ability, long-lived machinery, comfortable bank balances and the assurance of a peaceful, prosperous future.

To the progressive man, figures speak more forcibly than does the most persuasive lecturer on economic topics. The report of the United States Census for 1910 contains some figures that bear a distinct message to the farmers of the country. In 1900 the value of all farm property in the shape of farm implements and machinery was $749,775,970; in 1910 this same value had increased to $1,265,149,783, representing an increase of 68.7 per cent. This increase can be ascribed mainly to increased quantity rather than to higher prices, for the increase in price of farm machinery has been comparatively slight. It means that the farmers are realizing the benefits to be derived from the use of labor-saving machinery. In 1900 the acreage of improved land in farms was 414,498,487; in 1910 this became 478,451,750, an increase of only 15.4 per cent. These figures may be a little more significant if expressed in the following way: In 1900 there was $1.80 worth of machinery for each acre of improved farm land; in 1910 this had increased to $2.65, or an increase of over 47 per cent.

These figures will immediately indicate an opportunity for the furtherance of economic agriculture. With so much capital invested in equipment, the American farmer would certainly be a very bad business man indeed if he did not take some means of protecting this equipment to reduce depreciation and to increase its length of life. The question has sometimes been asked, does it pay to house farm machinery? Is it not a better practice not to give any special care to the machinery but use it as long as it will run without care then buy newer and more up-to-date equipment?

The situation bears some consideration. According to Census figures, the average investment per farm in farm machinery is almost exactly $200. This, however, is the case when every sort of farm is included, and since the Census Bureau’s definition of a farm is extremely liberal it would not be practical for our purposes. A fair estimate of the average value of farm machinery on a farm is $1,000. No reliable figures are available to indicate the rate of depreciation of farm machinery; one farmer will take excellent care of his binder and it may do service for twenty or twenty-five years, while another farmer will leave his binder in the middle of the field where the last stalk of grain was cut, and it would be surprising if his machine could operate satisfactorily for more than five seasons. To take ten years as the average life of farm machinery is certainly to be considered conservative.

Most farm machines are well and substantially constructed and will render satisfactory and efficient service with slight repairs for a much longer term of years than the average which has just been given. It is entirely safe to assume that the average length of efficient service can be increased to fifteen years providing proper care is given. It is almost equally safe to assume that the average life of uncared-for machinery will not be much more than five years.

The farmer who has a thousand dollars worth of machinery to which he gives no care and attention will then have an annual reduction in value of $200, besides his interest charge of $60 on his investment or a total debit of $260. The farmer who properly houses his machinery will have an annual deduction of $66.66 for depreciation and the same interest charge of $60. He will have, in addition, an annual charge of $25 for interest and depreciation on his building if it cost $250, or a total of $151.66, which is $108.34 less than that of his improvident neighbor. The careful farmer then may consider that he has in his implement house an investment representing over $1,800 as shown by the saving it brings him; as a simple implement shed can be built for $250, a net profit of an interest-paying $1,550 remains. Putting the problem in another way, on many farms the savings on machinery will pay for a shed in two or three years.

Fig. 3. Details of Simple Implement Shed

Only one wide sliding door is shown, though another smaller door can be inserted if desired. The truss construction shown in Fig. 10 is used above the wide door. Either vertical or horizontal siding may be used, the former being simple and satisfactory construction. The front wall may be omitted in localities where inclement weather is uncommon.

Fig. 4. Exterior of Open Type of Implement Shed

Fig. 5. Perspective of Framing of Open Type of Implement Shed

In view of the fact that the small tractor is becoming an extremely popular source of farm power, special consideration should be given to its shelter. The tractor is an implement that would be extremely likely to be injured as a result of exposure to weather. It is entirely possible that the damage which may be done to this one single machine in one winter’s exposure may be sufficient to pay for the cost of a machine shed which will house all the implements on the farm.

So much for the economic side. The figures that have just been given relate only to a very conservative case. On many farms the saving would be a great deal more. Besides this there are other things of which the value cannot be estimated, such as the benefit of having a machine that will operate when it is called upon to do so; the added value an implement shed gives to the farm; and the additional prestige which will redound to the owner of the farm.

The careful farmer will, of course, find that criticisms of ill-cared-for machinery do not apply to him; he has a machine shed, and knows the value of paint, oil, and grease in extending the life of implements. His equipment always looks new, for as rust breaks through the protecting coat of paint, a new coat is immediately applied; and his plowshares, discs, cultivator shovels, and other bright parts of implements are always given a thorough coating of grease before being put away for the winter. As a result, his implements are ready for business when spring comes and time is valuable.

## THE DESIGN OF THE BUILDING

In preparing the design for machine sheds one of the first considerations is that of economy. A machine shed is a building which is almost always used for no other purpose than to shelter machinery. It is not like a bin for the storage of grain where strength is an exceedingly important factor nor is it like a barn where so many operations are carried on within; consequently the simplest and cheapest structure that is consistent with reasonable durability is the one that is the most advisable. Wood is a product available in every section and is the cheapest and most suitable material for the construction of an implement shed.

Fig. 6. Details of Open Type of Implement Shed

Framing of 6x6 posts, thoroughly braced. Ends may be boarded or left open as desired. Foundation piers act as wheel guards. Width between posts can be varied to suit requirements.

Paint, the great preservative, should be applied to all
farm buildings. The initial cost of two coats of good paint is not prohibitive; the durability of the wood may be increased almost indefinitely if the surface is kept covered to prevent the ingress of the spores of decay. The prosperous farmer’s buildings are always kept painted, not only to preserve the wood, but to improve the appearance of the buildings themselves.

On new wood, two coats are usually sufficient. The first coat should contain mainly oil, with a small amount of the base and coloring pigments, so that it will permeate every pore; the second coat should be heavier, containing less oil and more pigment. Surfaces that have been painted can be kept in good condition by the occasional application of a single coat.

The planning of an implement shed will require data as to the number and size of machines and the amount of space that each will occupy. The arrangement of the machines so as to make them easily accessible at times when they are most needed is also important, e. g., a binder being used but once a year may well occupy a far corner, leaving a space near the door for the mower and plow, implements which are used oftener and for longer periods than the binder. The manure spreader, wagons and buggies are used so much throughout the year that they should be especially accessible. Table I, pages 19 and 20, gives the floor space required for most farm machines; the height of the machine is also given. Of course, it is entirely possible to crowd machines together as they are put into the shed, and so much saving in room can be accomplished in this way that little clearance space need be left. For instance, the outer edge of a binder platform can be easily raised several feet, provided a pair of reel slats with the attached arms are removed, and in this space beneath the platform can be stored such implements as hand drill, walking plows, etc. Similar opportunities for economy in space can very easily be found.

Fig. 7. Exterior of Wide Enclosed Implement Shed

Fig. 8. Perspective of Framing of Wide Enclosed Implement Shed

In general the construction of a machine shed is that of the very simplest; yet utility and beauty can be very easily combined with simplicity. Since the building is not subjected to any heavy load, as would be the case with a crib or a barn, the framing is just sufficiently strong to safely hold the wall and roof covering and to prevent collapse of the building from wind or snow and ice loads. Very often 2x4’s or 4x4’s constitute the studs or posts and no heavier stock is used throughout the building. In wide sheds it may be found
necessary to use larger stuff and especially in the plate above the wide doorway. A two-story machine shed will, of course, require heavier and more substantial framing, but a two-story shed is comparatively rare. A floor may or may not be used as the owner may desire. It is likely to prove somewhat expensive in first cost and in maintenance, though for convenience it is much to be desired, especially if any repair work is to be done in the building.

The roof may be of almost any style from the simple single pitch shed roof to the modified shed roof or the ordinary double pitch gable roof. It is desirable that the pitch should be not less than one-quarter in order to get the greatest life out of the shingles, which are likely to collect moisture and give shorter service where the pitch is quite flat. The foundation of a machine shed will naturally not be designed for great strength except in the case of a two-story structure, since the only load which it has to support is that of the superstructure itself. A footing 12 to 16 inches wide at the bottom and extending down a foot or 15 inches into solid soil will support a building of this kind. However, if a concrete floor is put in the building as is sometimes done in the more expensive ones, it will be well to extend the foundation wall and footing to a point below the frost line, which will vary from a foot to three feet according to climate.

Sills are usually not necessary in the simple framing of machine sheds. The posts can be set directly upon foundation walls and fastened in any one of many different ways that have been devised. Timbers are more subject to decay at the ends than elsewhere, consequently it is advisable to treat them at this point with a preservative such as creosote. This will add greatly to the durability. The foundation wall should be brought up some distance above the ground so as to further protect the bottom timbers from moisture. This above-ground extension must be omitted at doorways.

Fig. 9. Details of a Wide Enclosed Implement Shed

Strong framing is necessary to insure durability in this structure. Members may be solid or built up. Details of one form of roof truss are shown in Fig. 11. Note solid foundation. Doors may be located to suit requirements.

One of the most serious problems in the design of a machine shed is the insertion of doors. Wide doors are an absolute necessity, especially for certain machines. An eight-foot door is large enough for the majority of farm machines, even allowing the modern binder with its folding grain dividers to enter in safety. The wide drill, the rake, and several other implements require a much wider door than this and it may be necessary to provide an opening 12 or even 14 feet wide. This leaves a long unsupported section
of the plate directly above the doorway. To keep it and the roof from sagging, special provision must be made either by putting in an exceptionally strong plate at this point, by building up a small wooden truss, or by making a truss of wood and iron as shown in the illustration. (Fig. 10.)

The doors themselves should be very solidly and substantially made. It is a matter of good practice to have as few doors as possible. In the average machine shed one 8-foot door and one 12 or 14-foot door are sufficient to meet requirements. A door wider than four feet should not be swung on hinges under any circumstances, as it is sure to pull out the hinges or to sag very badly. Sliding doors of good construction are to be recommended in preference to hinged doors (Fig. 12). It is entirely possible to make a good close-fitting door of this type and there need never be any trouble in its operation.

The use of other buildings for the storage of farm implements is not a desirable procedure except in certain instances, such as keeping wagons in the driveway of cribs, leaving the spreader at the end of an alleyway of a barn for convenience in loading, etc. In general, other buildings are much more expensive than a machine shed and those portions of them devoted to the storage of farm implements could in most cases be more profitably used, especially when the very small unit floor-space cost of a machine shed is taken into consideration. Then, too, if a special place is not provided for the implements, the farm animals may come in contact with them, causing injury of the animals or damage to the machines.

## REPRESENTATIVE TYPES OF SHEDS

### The Simple Shed Type.

The needs of the average farm for a cheap, easily built implement shed are met by this building. Illustrations of this type of shed are shown in Figs. 1, 2 and 3. The framing consists of 6x6 posts set on a light 1:2½:5 mixture concrete foundation at intervals of eight feet, the plate consisting of two 2x6’s. Short diagonal braces can be set in underneath between the plate and the post in order to give the plate further support. The rafters for a span of 18 feet should be at least 2x6 and better 2x8, set not less than two feet apart on centers. The wall covering may consist of vertical siding, either 10 or 12-inch boards, with the cracks covered by ogee battens. For horizontal siding,
studs are necessary; these should be 2x4’s, placed not over 3 feet apart. Either drop-siding, German or novelty siding or ordinary weather-boarding may be used satisfactorily, but the latter is somewhat light for a building of this kind and would probably not be as durable as the others mentioned.

Fig. 10. Detail of Truss Over Large Doors in Implement Shed

Fig. 11. Roof Truss Details

The upper illustration (Fig. 10) shows a method of building a truss above wide doors to prevent sagging of roof. It may be varied to suit circumstances.

The roof trusses shown in Fig. 11 suggest methods of framing for wide sheds, as in Fig. 3 and Fig. 9.

The building may be entirely enclosed, having the doors on the high side. The practice of enclosing the building entirely is generally to be recommended, though sometimes for the sake of economy and convenience and in localities where the winds are very constant in their direction, it may be advisable to omit part of the exterior wall covering, leaving one side open, this side being the one opposite to the direction from which the prevailing winds come.

### The Open Shed Type.

Under some circumstances the open shed type of building (shown in Figs. 4, 5 and 6) will be the more suitable. This is especially true where wagons, racks and spreaders are used frequently. The framing of the building consists simply of 6x6 posts set on concrete piers at intervals of 9 feet. On these are set 2x6 rafters supporting a double pitched gable roof. The building is opened on both sides but both ends may be enclosed.

This building is extremely convenient, although it does not give very thorough protection to the machines. A wagon or spreader can be driven directly through one of the bays and horses unhitched outside. With a building 18 feet wide and eaves overhanging one foot, the implements will be protected from all but driving rains, though sweeping snow will have free access to the interior. The posts are placed nine feet apart in order to provide sufficient room for driving a team through. It may be possible to reduce this dimension to eight feet, or to increase it to 10 feet in case a three-horse team is to be driven through. The concrete piers supporting the posts are made conical in shape, acting thus as wheel guards to prevent the hubs of the wheels from striking the posts.

One or more bays of the shed may be enclosed if desired to give adequate shelter to machines, such as mowers, binders, etc., which would suffer from exposure. Of course, the shed as well as the preceding one can be built to any length desired, though a building more than four times as long as it is wide will present a somewhat peculiar appearance on account of the long, low roof line.

Fig. 12. Construction Details

These details apply in general to the implement shed plans. The girder splice shown makes a firm, solid joint. If double hung sash are used, standard window framing is employed, as shown. Wide doors are always hung on a track; the detail shows weather strip at top, and bracket with roller at bottom to keep door from swinging out.

### The Wide Enclosed Type.

A better and a little more expensive type of implement shed, yet one perhaps better suited to the average farm is shown in Figs. 7, 8 and 9. This shed is made 26 feet in width and as long as may be necessary, although a building 26x40 will usually be found sufficiently large to house the machines on the average general-purpose farm. The framing of this shed is a little more substantial than in the types previously discussed, consisting of 6x6’s with 4x6 plates. Should horizontal siding be used, it will naturally follow that instead of using these posts, 2x4 studs will be employed as previously described in the simple shed type on page thirteen. The height of the walls should be not less than 10 feet, which with the gable roof will make the building a little more attractive in appearance than the one previously described. A span of 26 feet is almost too great for the adequate support of the roof unless some device such as truss bracing and purline is used to give the rafters additional stiffness. (Fig. 11.)

Experience has shown that the two widths—18 feet and 26 feet are peculiarly adaptable to the dimensions of the various farm machines. Using the 26-foot width, considerable opportunity is given for the utilization of the floor space, since a wider floor area unsupported by posts is available. As far as possible, interior posts should be avoided, for they interfere very seriously in the placing and moving of machinery.

### The Two-Story Type.

As stated before, the use of a two-story machine shed is rather rare, for two reasons: First, the additional expense in material and labor, and, Second, the difficulty of getting machines up to the second floor. The only advantage that is gained is the doubling of the floor space under the same roof.

Fig. 13. Details of Two-Story Implement Shed

The framing in this type of shed must be unusually strong and substantial. The girders and, in fact, all framing members, may be either solid or built up. A central post is necessary in each framing unit.

The construction of the building (illustrated in Figs. 13, 14 and 15) will necessarily be rather substantial. The framing may consist of 6x6 posts and 4x6 girts, which should be securely joined in order to give rigidity to the structure. The girts are located at vertical intervals of not to exceed 5 feet, so as to afford good nailing for vertical siding. If horizontal siding is used, the girts may be spaced wider, say, one each at the top, bottom, and middle of the post, while 2x6 studs are set in on which to nail the boards. Diagonal bracing is a decided advantage. The building may be constructed either 18 or 26 feet wide, and it is seldom that a
building longer than 40 feet will be necessary. The foundation should be much more substantial than in the types previously described. It should extend well below the frost line and be almost as strong as that used for barns.

The second floor will be used for the storage of the lighter machines such as small plows, harrows, drills and all the lighter tools which make up the farmer’s equipment; while the first floor will be utilized for the storage of the heavier machines such as binders, wagons, etc. Getting the lighter machines up to the second floor may be accomplished in one of two ways. An ordinary block and tackle can be utilized either through an outside door in the gable of the roof or through a hole in the floor in the interior of the building. If space is available the construction of a rather steep runway outside the building and leading to the second floor may be advantageous. This runway can be constructed of rather light material, using a pair of 4x6’s for joists, and flooring them with rough 2-inch stuff. An angle of 30 degrees with the horizontal will make it possible to pull machines up the runway with only a small amount of labor. This arrangement has been found to be superior to the use of a hoist. It can be used to the best advantage when the shed is located on the slope of a rather steep hill.

TABLE I.

Floor Space and Height of Space Required to House Common Farm Implements.

Implements— | Floor Space in Feet | Height of Space in Feet
--- | --- | ---
Plows—
Walking | 8x3 |  | 3 |
Sulky and horse gang (tongue off; add 10 ft. for tongue) | 8x6 |  | 4 |
Engine gang | 16x7 |  | 5 |
Harrows—
Spike tooth, per section | 5x5 |  | 2 |
Spring tooth, per section | 5x4 |  | 1 | ½
Single disc, 8 ft. with truck (tongue off) | 6x9 |  | 4 |
Double disc, 7 ft. with truck (tongue off) | 8x8 |  | 4 |
Weeder—
(Thills on) | 13x8 |  | 4 |
Grain Drills—
12x7 (tongue off; add 10 ft. for tongue) | 5x8 |  | 5 |
16x7 with press attachment (tongue off) | 7x11 |  | 5 |
Rollers—
Smooth | 3x10 |  | 4 | ½
Corrugated, single (tongue off; add 10 ft. for tongue) | 3x10 |  | 4 |
Corrugated, double | 4x8 |  | 4 |
Corn Planter—
Two row (tongue off; add 10 ft. for tongue) | 5½x6 |  | 3 | ½
Cultivators—
Walking, one horse | 7x2 |  | 3 | ½
Riding, single row (tongue off; add 10 ft. for tongue) | 8x5 |  | 4 |
Riding, two row (tongue off; add 10 feet for tongue) | 8x10 |  | 4 |
Alfalfa (tongue off; add 10 ft. for tongue) | 7x6 |  | 5 |
Mower—
6 ft. (tongue off; add 10 ft. for tongue) | 5x6 |  | 7 |
Binders—
Grain, 8 ft. (tongue truck off) | 8x14 |  | 7 |
Grain, 6 ft. (tongue truck off) | 8x12 |  | 7 |
Corn (tongue off; add 11 ft. for tongue) | 13x6 |  | 7 |
Hay Rakes—
Self-dump (thills off) | 5½x11 | ½ | 5 |
Side-delivery (tongue off; add 10 ft. for tongue) | 13x9 |  | 5 |
Tedders—
Kicker (tongue off; add 8 ft. for tongue) | 5½x8 |  | 5 |
Combination (see side-delivery rakes)
Hay Loader | 14x9 | ½ | 9 |
Ensilage Cutter, 20-ton (tongue off) | 11x5 | ½ | 7 |
Corn Shredder, 8 roll | 20x8 |  | 9 |
Corn Sheller | 20x8 |  | 11 |
Hay Press | 16x6 |  | 6 |
Grain Separator, 32-inch | 26x8 |  | 8 | ½
Clover Huller | 24x8 |  | 8 |
Gasoline Tractor, 20-4 H. P. | 15x9 |  | 9 |
Gasoline Tractor, 10-20 H. P. | 12x8 |  | 8 |
Portable Engine, 6 H. P. | 9x5 |  | 6 |
Fanning Mill, 24-inch | 4x3 | ½ | 5 |
Wagons—
Farm gear (tongue off; add 10 ft. for tongue) | 11x5 | ½ | 4 |
Wagon with box and top (tongue off) | 11x5 | ½ | 5 | ½
Wagon with box and tip top (tongue off) | 11x5 | ½ | 6 | ½
Wagon with hay rack (tongue off) | 16x7 | ½ | 5 |
Buggies—
One seated (thills up) | 8x5 | ½ | 7 |
Two seated (tongue off) | 10x5 | ½ | 8 |
Grain Dump (knocked down) | 12x4 |  | 4 |
Potato Machinery—
Planter (tongue off; add 9 ft. for tongue) | 5x3 |  | 4 |
Sprayer, two wheeled barrel (thills off) | 6x6 |  | 5 |
Digger, wheeled, elevator (tongue off) | 13x4 |  | 3 |
Automobiles—
Small | 11x6 |  | 7 |
Large | 14x7 |  | 8 |
Phosphorus Distributor, 1,000 lbs. (tongue off; add 10 ft. for tongue) | 4x10 |  | 4 |
Manure Spreader, 50 bu. (tongue off; add 10 ft. for tongue) | 17x7 |  | 6 |

THIS?

Fig. 14. Exterior of Two-Story Implement Shed

Fig. 15. Perspective of Framing of Two-Story Implement Shed

OR THIS?

The Automobile and Family Carriage Are Kept Under Cover. Is This Fair to the Implements Which Make the Farm Pay?

Fig. 16

Courtesy Tractor Farming.

“When it comes to actual waste, the Great American Desert with its constant canopy of blue sky over it has very little on the Great American Machine Shed. The chief difference is that the former is found in a particular locality only, while the latter extends from coast to coast. Both are in the open, both represent zero in profitable and economical usage, and both need the undivided attention of conservation experts.”—Tractor Farming.

Wood “Where Best”

The legitimate use of lumber where it is best, or by proper selection or treatment can be made to serve economically and safely, is the aim of the lumbermen in publishing a series of bulletins on Farm Structures. Wood has for so long been the most widely used building material that its availability and importance have either been taken for granted or lost sight of. It is helpful to review the outstanding features of the present situation:

Wood remains the most universal, most adaptable building material in the world.

The supply is ample for all requirements, and the kinds and grades best suited for all purposes are obtainable everywhere.

In cost it remains one of the cheapest materials.

It is the lightest building material known, and the strongest, weight for weight.

Its qualities are known; it is easy to work; it can be cut and shaped by any one into the myriad uses required for the shelter and comfort of man.

There is no material more beautiful in appearance, more susceptible to artistic finish, nor which is as productive of sentiment and satisfaction for home building.

Wood is a non-conductor of heat,—cool in summer and warm in winter.

The relative qualities of durability, serviceability and workability should be considered in selecting wood for homes and farm buildings. Consult the local lumber dealer. His knowledge and advice will assure cheaper, more stable buildings.

Except where naturally durable woods are available, a preservative treatment will prove economical for timber exposed to moisture and decay, as sills, basement flooring, fence posts; and in similar situations.

Other Farm Bulletins.

Other Bulletins in this series are upon:

Dairy and General Purpose Barns
Garages
Poultry Houses
Farm Residences

Ice Houses
Silos
Grain Storage Buildings
Swine Houses

The Preservative Treatment of Farm Timbers

Ask for those that will be helpful to you. Address:

NATIONAL LUMBER MANUFACTURERS
ASSOCIATION
Lumber Exchange
CHICAGO

*** END OF THE PROJECT GUTENBERG EBOOK IMPLEMENT SHEDS ***
Updated editions will replace the previous one—the old editions will be renamed.
Creating the works from print editions not protected by U.S. copyright law means that no one owns a United States copyright in these works, so the Foundation (and you!) can copy and distribute it in the United States without permission and without paying copyright royalties. Special rules, set forth in the General Terms of Use part of this license, apply to copying and distributing Project Gutenberg™ electronic works to protect the PROJECT GUTENBERG™ concept and trademark. Project Gutenberg is a registered trademark, and may not be used if you charge for an eBook, except by following the terms of the trademark license, including paying royalties for use of the Project Gutenberg trademark. If you do not charge anything for copies of this eBook, complying with the trademark license is very easy. You may use this eBook for nearly any purpose such as creation of derivative works, reports, performances and research. Project Gutenberg eBooks may be modified and printed and given away—you may do practically ANYTHING in the United States with eBooks not protected by U.S. copyright law. Redistribution is subject to the trademark license, especially commercial redistribution.
START: FULL LICENSE

## THE FULL PROJECT GUTENBERG™ LICENSE

PLEASE READ THIS BEFORE YOU DISTRIBUTE OR USE THIS WORK
To protect the Project Gutenberg™ mission of promoting the free distribution of electronic works, by using or distributing this work (or any other work associated in any way with the phrase “Project Gutenberg”), you agree to comply with all the terms of the Full Project Gutenberg License available with this file or online at www.gutenberg.org/license.
Section 1. General Terms of Use and Redistributing Project Gutenberg electronic works
1.A. By reading or using any part of this Project Gutenberg electronic work, you indicate that you have read, understand, agree to and accept all the terms of this license and intellectual property (trademark/copyright) agreement. If you do not agree to abide by all the terms of this agreement, you must cease using and return or destroy all copies of Project Gutenberg electronic works in your possession. If you paid a fee for obtaining a copy of or access to a Project Gutenberg electronic work and you do not agree to be bound by the terms of this agreement, you may obtain a refund from the person or entity to whom you paid the fee as set forth in paragraph 1.E.8.
1.B. “Project Gutenberg” is a registered trademark. It may only be used on or associated in any way with an electronic work by people who agree to be bound by the terms of this agreement. There are a few things that you can do with most Project Gutenberg electronic works even without complying with the full terms of this agreement. See paragraph 1.C below. There are a lot of things you can do with Project Gutenberg electronic works if you follow the terms of this agreement and help preserve free future access to Project Gutenberg electronic works. See paragraph 1.E below.
1.C. The Project Gutenberg Literary Archive Foundation (“the Foundation” or PGLAF), owns a compilation copyright in the collection of Project Gutenberg electronic works. Nearly all the individual works in the collection are in the public domain in the United States. If an individual work is unprotected by copyright law in the United States and you are located in the United States, we do not claim a right to prevent you from copying, distributing, performing, displaying or creating derivative works based on the work as long as all references to Project Gutenberg are removed. Of course, we hope that you will support the Project Gutenberg mission of promoting free access to electronic works by freely sharing Project Gutenberg works in compliance with the terms of this agreement for keeping the Project Gutenberg name associated with the work. You can easily comply with the terms of this agreement by keeping this work in the same format with its attached full Project Gutenberg License when you share it without charge with others.
1.D. The copyright laws of the place where you are located also govern what you can do with this work. Copyright laws in most countries are in a constant state of change. If you are outside the United States, check the laws of your country in addition to the terms of this agreement before downloading, copying, displaying, performing, distributing or creating derivative works based on this work or any other Project Gutenberg work. The Foundation makes no representations concerning the copyright status of any work in any country other than the United States.
1.E. Unless you have removed all references to Project Gutenberg:
1.E.1. The following sentence, with active links to, or other immediate access to, the full Project Gutenberg License must appear prominently whenever any copy of a Project Gutenberg work (any work on which the phrase “Project Gutenberg” appears, or with which the phrase “Project Gutenberg” is associated) is accessed, displayed, performed, viewed, copied or distributed:

> This eBook is for the use of anyone anywhere in the United States and most other parts of the world at no cost and with almost no restrictions whatsoever. You may copy it, give it away or re-use it under the terms of the Project Gutenberg™ License included with this eBook or online at www.gutenberg.org. If you are not located in the United States, you will have to check the laws of the country where you are located before using this eBook.

1.E.2. If an individual Project Gutenberg electronic work is derived from texts not protected by U.S. copyright law (does not contain a notice indicating that it is posted with permission of the copyright holder), the work can be copied and distributed to anyone in the United States without paying any fees or charges. If you are redistributing or providing access to a work with the phrase “Project Gutenberg” associated with or appearing on the work, you must comply either with the requirements of paragraphs 1.E.1 through 1.E.7 or obtain permission for the use of the work and the Project Gutenberg trademark as set forth in paragraphs 1.E.8 or 1.E.9.
1.E.3. If an individual Project Gutenberg electronic work is posted with the permission of the copyright holder, your use and distribution must comply with both paragraphs 1.E.1 through 1.E.7 and any additional terms imposed by the copyright holder. Additional terms will be linked to the Project Gutenberg License for all works posted with the permission of the copyright holder found at the beginning of this work.
1.E.4. Do not unlink or detach or remove the full Project Gutenberg License terms from this work, or any files containing a part of this work or any other work associated with Project Gutenberg.
1.E.5. Do not copy, display, perform, distribute or redistribute this electronic work, or any part of this electronic work, without prominently displaying the sentence set forth in paragraph 1.E.1 with active links or immediate access to the full terms of the Project Gutenberg License.
1.E.6. You may convert to and distribute this work in any binary, compressed, marked up, nonproprietary or proprietary form, including any word processing or hypertext form. However, if you provide access to or distribute copies of a Project Gutenberg work in a format other than “Plain Vanilla ASCII” or other format used in the official version posted on the official Project Gutenberg website (www.gutenberg.org), you must, at no additional cost, fee or expense to the user, provide a copy, a means of exporting a copy, or a means of obtaining a copy upon request, of the work in its original “Plain Vanilla ASCII” or other form. Any alternate format must include the full Project Gutenberg License as specified in paragraph 1.E.1.
1.E.7. Do not charge a fee for access to, viewing, displaying, performing, copying or distributing any Project Gutenberg works unless you comply with paragraph 1.E.8 or 1.E.9.
1.E.8. You may charge a reasonable fee for copies of or providing access to or distributing Project Gutenberg electronic works provided that:

- • You pay a royalty fee of 20% of the gross profits you derive from the use of Project Gutenberg works calculated using the method you already use to calculate your applicable taxes. The fee is owed to the owner of the Project Gutenberg trademark, but he has agreed to donate royalties under this paragraph to the Project Gutenberg Literary Archive Foundation. Royalty payments must be paid within 60 days following each date on which you prepare (or are legally required to prepare) your periodic tax returns. Royalty payments should be clearly marked as such and sent to the Project Gutenberg Literary Archive Foundation at the address specified in Section 4, “Information about donations to the Project Gutenberg Literary Archive Foundation.”
- • You provide a full refund of any money paid by a user who notifies you in writing (or by e-mail) within 30 days of receipt that s/he does not agree to the terms of the full Project Gutenberg™ License. You must require such a user to return or destroy all copies of the works possessed in a physical medium and discontinue all use of and all access to other copies of Project Gutenberg™ works.
- • You provide, in accordance with paragraph 1.F.3, a full refund of any money paid for a work or a replacement copy, if a defect in the electronic work is discovered and reported to you within 90 days of receipt of the work.
- • You comply with all other terms of this agreement for free distribution of Project Gutenberg™ works.

1.E.9. If you wish to charge a fee or distribute a Project Gutenberg™ electronic work or group of works on different terms than are set forth in this agreement, you must obtain permission in writing from the Project Gutenberg Literary Archive Foundation, the manager of the Project Gutenberg™ trademark. Contact the Foundation as set forth in Section 3 below.
1.F.
1.F.1. Project Gutenberg volunteers and employees expend considerable effort to identify, do copyright research on, transcribe and proofread works not protected by U.S. copyright law in creating the Project Gutenberg™ collection. Despite these efforts, Project Gutenberg™ electronic works, and the medium on which they may be stored, may contain “Defects,” such as, but not limited to, incomplete, inaccurate or corrupt data, transcription errors, a copyright or other intellectual property infringement, a defective or damaged disk or other medium, a computer virus, or computer codes that damage or cannot be read by your equipment.
1.F.2. LIMITED WARRANTY, DISCLAIMER OF DAMAGES - Except for the “Right of Replacement or Refund” described in paragraph 1.F.3, the Project Gutenberg Literary Archive Foundation, the owner of the Project Gutenberg™ trademark, and any other party distributing a Project Gutenberg™ electronic work under this agreement, disclaim all liability to you for damages, costs and expenses, including legal fees. YOU AGREE THAT YOU HAVE NO REMEDIES FOR NEGLIGENCE, STRICT LIABILITY, BREACH OF WARRANTY OR BREACH OF CONTRACT EXCEPT THOSE PROVIDED IN PARAGRAPH 1.F.3. YOU AGREE THAT THE FOUNDATION, THE TRADEMARK OWNER, AND ANY DISTRIBUTOR UNDER THIS AGREEMENT WILL NOT BE LIABLE TO YOU FOR ACTUAL, DIRECT, INDIRECT, CONSEQUENTIAL, PUNITIVE OR INCIDENTAL DAMAGES EVEN IF YOU GIVE NOTICE OF THE POSSIBILITY OF SUCH DAMAGE.
1.F.3. LIMITED RIGHT OF REPLACEMENT OR REFUND - If you discover a defect in this electronic work within 90 days of receiving it, you can receive a refund of the money (if any) you paid for it by sending a written explanation to the person you received the work from. If you received the work on a physical medium, you must return the medium with your written explanation. The person or entity that provided you with the defective work may elect to provide a replacement copy in lieu of a refund. If you received the work electronically, the person or entity providing it to you may choose to give you a second opportunity to receive the work electronically in lieu of a refund. If the second copy is also defective, you may demand a refund in writing without further opportunities to fix the problem.
1.F.4. Except for the limited right of replacement or refund set forth in paragraph 1.F.3, this work is provided to you ‘AS-IS’, WITH NO OTHER WARRANTIES OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO WARRANTIES OF MERCHANTABILITY OR FITNESS FOR ANY PURPOSE.
1.F.5. Some states do not allow disclaimers of certain implied warranties or the exclusion or limitation of certain types of damages. If any disclaimer or limitation set forth in this agreement violates the law of the state applicable to this agreement, the agreement shall be interpreted to make the maximum disclaimer or limitation permitted by the applicable state law. The invalidity or unenforceability of any provision of this agreement shall not void the remaining provisions.
1.F.6. INDEMNITY - You agree to indemnify and hold the Foundation, the trademark owner, any agent or employee of the Foundation, anyone providing copies of Project Gutenberg™ electronic works in accordance with this agreement, and any volunteers associated with the production, promotion and distribution of Project Gutenberg™ electronic works, harmless from all liability, costs and expenses, including legal fees, that arise directly or indirectly from any of the following which you do or cause to occur: (a) distribution of this or any Project Gutenberg work, (b) alteration, modification, or additions or deletions to any Project Gutenberg work, and (c) any Defect you cause.
Section 2. Information about the Mission of Project Gutenberg
Project Gutenberg is synonymous with the free distribution of electronic works in formats readable by the widest variety of computers including obsolete, old, middle-aged and new computers. It exists because of the efforts of hundreds of volunteers and donations from people in all walks of life.
Volunteers and financial support to provide volunteers with the assistance they need are critical to reaching Project Gutenberg’s goals and ensuring that the Project Gutenberg collection will remain freely available for generations to come. In 2001, the Project Gutenberg Literary Archive Foundation was created to provide a secure and permanent future for Project Gutenberg and future generations. To learn more about the Project Gutenberg Literary Archive Foundation and how your efforts and donations can help, see Sections 3 and 4 and the Foundation information page at www.gutenberg.org.
Section 3. Information about the Project Gutenberg Literary Archive Foundation
The Project Gutenberg Literary Archive Foundation is a non-profit 501(c)(3) educational corporation organized under the laws of the state of Mississippi and granted tax exempt status by the Internal Revenue Service. The Foundation’s EIN or federal tax identification number is 64-6221541. Contributions to the Project Gutenberg Literary Archive Foundation are tax deductible to the full extent permitted by U.S. federal laws and your state’s laws.
The Foundation’s business office is located at 41 Watchung Plaza #516, Montclair NJ 07042, USA, +1 (862) 621-9288. Email contact links and up to date contact information can be found at the Foundation’s website and official page at www.gutenberg.org/contact
Section 4. Information about Donations to the Project Gutenberg Literary Archive Foundation
Project Gutenberg™ depends upon and cannot survive without widespread public support and donations to carry out its mission of increasing the number of public domain and licensed works that can be freely distributed in machine-readable form accessible by the widest array of equipment including outdated equipment. Many small donations ($1 to $5,000) are particularly important to maintaining tax exempt status with the IRS.
The Foundation is committed to complying with the laws regulating charities and charitable donations in all 50 states of the United States. Compliance requirements are not uniform and it takes a considerable effort, much paperwork and many fees to meet and keep up with these requirements. We do not solicit donations in locations where we have not received written confirmation of compliance. To SEND DONATIONS or determine the status of compliance for any particular state visit www.gutenberg.org/donate.
While we cannot and do not solicit contributions from states where we have not met the solicitation requirements, we know of no prohibition against accepting unsolicited donations from donors in such states who approach us with offers to donate.
International donations are gratefully accepted, but we cannot make any statements concerning tax treatment of donations received from outside the United States. U.S. laws alone swamp our small staff.
Please check the Project Gutenberg web pages for current donation methods and addresses. Donations are accepted in a number of other ways including checks, online payments and credit card donations. To donate, please visit: www.gutenberg.org/donate.
Section 5. General Information About Project Gutenberg electronic works
Professor Michael S. Hart was the originator of the Project Gutenberg concept of a library of electronic works that could be freely shared with anyone. For forty years, he produced and distributed Project Gutenberg eBooks with only a loose network of volunteer support.
Project Gutenberg eBooks are often created from several printed editions, all of which are confirmed as not protected by copyright in the U.S. unless a copyright notice is included. Thus, we do not necessarily keep eBooks in compliance with any particular paper edition.
Most people start at our website which has the main PG search facility: www.gutenberg.org.
This website includes information about Project Gutenberg, including how to make donations to the Project Gutenberg Literary Archive Foundation, how to help produce our new eBooks, and how to subscribe to our email newsletter to hear about new eBooks.