## The Project Gutenberg eBook of How to Make Draperies

This eBook is for the use of anyone anywhere in the United States and most other parts of the world at no cost and with almost no restrictions whatsoever. You may copy it, give it away or re-use it under the terms of the Project Gutenberg License included with this eBook or online at www.gutenberg.org. If you are not located in the United States, you will have to check the laws of the country where you are located before using this eBook.

Title: How to Make Draperies

Creator: Singer Sewing Machine Company

Release date: September 24, 2020 [eBook #63282]
Most recently updated: October 18, 2024

Language: English

Other information and formats: www.gutenberg.org/ebooks/63282

Credits: Produced by Stephen Hutcheson and the Online Distributed
Proofreading Team at https://www.pgdp.net

*** START OF THE PROJECT GUTENBERG EBOOK HOW TO MAKE DRAPERIES ***

29c

# How to Make
Draperies

Instructions for
  • Fabrics
  • Color
  • Design
  • Measurements
  • Construction

Published by
THE SINGER COMPANY

Book No. 102

1

# How to Make
Draperies

CONTENTS page
Fabrics 3
Color and Design 7
Selection of Needles and Thread 8
Window Measurements 11
Construction Details 15
Measuring for Pleats 26

Copyright© 1960 by The Singer Company

Copyright under International Copyright Union • All Rights Reserved under Inter-America Copyright Union • No part of this book may be reproduced in any manner whatsoever without written permission.

2
3

## Fabrics

Drapery fabrics are available to us today in an overwhelming variety for every decor—not only in the traditional fabrics, but also in the many new synthetics and blends.

Whether the room is traditional, modern, formal or informal, you need only visit the drapery fabric department to realize what a wide choice of fabrics are available in either group.

Windows are so much a part of the background that the fabric chosen, its texture, color and line, and the design of the curtains, draperies and slip covers must be in keeping with the atmosphere of the room and contribute to the over-all effect.

For the very formal treatment, you’ll want to choose something in the Damask designs, taffetas, moires, brocades, satins, brocatelles or the many blends of the pure and man-made fibers, some with metallic threads woven in. Fringes and tassels are used as trims, and the window treatment would include draped valances, swags, cascades, elaborate cornices, tie-backs, etc.

For the less formal or informal 4 room, the choice of fabric is even wider—linens in medium and sheer weights, prints and lacey patterns, marquisette, scrim, voile, ninon, denim, sailcloth, chintz, polished cotton, antique satin, organdy, batiste and many blends of synthetics, such as Fortisan and rayon or silk. The curtain treatment should be simple. If valances are used, they should be plain with straight lines.

Many of the new synthetic fibers are a real advantage to the home-maker because of their easy washing and quick drying properties. Some require very little pressing, if any.

In estimating the yardage required, consider the length of the drapery, before finishing hems and heading, and the width of the window or space to be covered. An allowance of 2½ or 3 times the width should be made for fullness. When using sheer fabrics, draperies should be full enough to hang in easy, graceful folds. Over-curtains or draperies of medium weight fabrics require a fullness of 2 to 2½ times the width. Also, if you select a fabric with a large one-way design, some allowance should be made for matching the design so all lengths will balance.

For example: The window is 64″ wide which requires 4 widths of 48″ wide fabric for a 3 to 1 fullness. The drapery lengths are 2⅓ yards long. If a plain fabric or overall design is used, the fabric required would be 9⅓ yards, but if the fabric has a 24″ repeat pattern, you must allow 1⅓ yards more, or a total of 10⅔ yards for matching the design.

Consider the width of the fabric when figuring the number of widths for fullness. Some fabrics are only 36″ wide—chintz and some polished cottons, for example. Others may run 40″—48″—even 54″ or 60″ in width; but the average is about 48″ wide.

Grain lines of fabric.

⇐Crosswise Grain—Weft or Filling⇒
⇐Lengthwise Grain—Warp⇒
⇐True Bias⇒

5

Draperies must be cut on the true lengthwise and crosswise grain of the fabric so that when hung, they fall straight from the rod in even, graceful folds.

In weaving, yarns are threaded lengthwise on a loom which form the warp of the fabric. Another yarn is interlaced back and forth crosswise and is called the weft or filling thread. This is known as the plain weave. Linen, voile, chintz, etc., are a few of the plain woven fabrics. There are variations of the plain weave, such as the pile weave, with velveteen and corduroy as examples. The basket weave is another, with Monk’s cloth as an example. The diagonal line halfway between the lengthwise and crosswise threads is the bias of the fabric.

The twill weave is perhaps one of the most durable. The filling yarn forms a diagonal line, passing over one warp yarn and under two or more. Denim, drill cloth and ticking are examples of this weave.

The satin weave is an irregular weave where one yarn passes over several yarns of the other set before interweaving, forming a floating, lustrous surface.

Weaves are used in combinations to obtain the various patterns in Damasks, brocades, Jacquards, etc.

Cutting on true crosswise grain.

6

The yarns made from the different fibers—the natural, man-made and blended fibers—are of various sizes, weights, smoothness and fuzziness. The type of yarns used in the different weaves influences the texture of the fabric as well as its weight, lustre and durability.

When cutting drapery lengths, be sure to start with a true crosswise grain. Most firmly woven plain weave fabrics can be torn. Snip the selvage before you tear the fabric. Linens, loosely woven and nubby fabrics, novelty weaves and many others will not tear satisfactorily. To straighten these, it is necessary to pull a thread crosswise and cut on pulled line.

After cutting lengths, check to see if the ends of the fabric are square. If not, square the crosswise edge by pulling the low corner on a true bias from opposite side of the fabric. Sometimes dampening the fabric will relax the threads and make straightening easier.

#### ESTIMATE OF YARDAGE

DRAPERIES
Full Length Window—48″ Material | 6 | YARDS
Full Length Window with Valance | 6½ | ″
LINING—Full Length Window | 5¼ | ″

> These figures are the approximate requirements. Always, where possible, take careful measurements for more accurate estimate. It is much better to have extra material than not enough.

> When using materials with a large floral pattern or plaid, allow one full length of the motif for each additional length required for draperies.

7

## Color and Design

Color has a language all its own—It expresses, it soothes, it stimulates, it creates; it can give you a lift. And color as a home decorator can be made to work like magic. With color, the dullest rooms can be made to sparkle with warmth and good cheer. Any color scheme is good as long as it is balanced and it pleases you. A number of colors, tints and shades may be used in one room, but one color should be dominant and it should be used in different areas of the room. The second color should be subordinate, not of the same value. Then a third color may be used for accent or contrast. The neutral colors: gray, white and black, are good background or accent colors.

Do not overlook the possibilities of accessories, such as pillows, vases, china, lamps and books to supply an accent color to complete your color scheme.

Your color scheme may be taken from a favorite picture, a family heirloom or may express the interests and personalities of the family. Consider also the location of the room—East, West, North or South—and how the light enters the room.

There are three primary colors—red, yellow and blue. These colors are mixed to obtain secondary colors. For example, red and yellow produce the color orange; red and blue, the color violet and blue and yellow, the color green. By blending these six colors we complete the color wheel which is made up of 8 red, red orange, orange, yellow, yellow green, green, blue green, blue, blue violet and violet.

We refer to certain colors as warm, others as cool and still others as neither warm nor cool. The warm colors are red, yellow and orange. The cool colors are the blues. Green is neither warm nor cool but if mixed with yellow, it becomes warm; when mixed with blue, it becomes a cool color.

Color and line apparently change the size of the room. Cool, light colors and vertical lines make walls appear higher and the room larger, while warm colors and horizontal lines seem to lower the ceiling and draw the walls nearer.

For North and East rooms, use warm colors. If little light enters in, use light shades of the warm colors. Use the cool colors in rooms with South or West exposures.

When purchasing your fabrics for curtains, draperies and slip covers, keep in mind the overall effect. Consider the room exposure, light, size of room, furniture arrangement and what color and design will do to create a room you will always enjoy. Since windows are a very important part of the room as a unit, the fabric chosen for curtains or draperies should also be used to slip cover a sofa or chair, a dressing table cover, or a dust ruffle for the bed.

### Selection of Needles and Thread

Sewing thread should blend as nearly as possible with the fabric in color, fiber and size. Silk and wool fabrics are stitched with silk thread. Cottons, linens and some blended fabrics are stitched with cotton thread or mercerized thread. The synthetic fabrics and blends of the pure and man-made fibers may be stitched with silk, mercerized 9 cotton, nylon or Dacron (DuPont) thread. The needle is selected with consideration to both the thread and the fabric.

With fabrics used for glass curtains and for sheer curtains, such as organdy, voile, “Dacron,” dotted Swiss, marquisettes, batiste and sheer linen, use a fine cotton thread, size 80 or 90, or a mercerized thread. Use a size 14 needle for mercerized thread and a size 11 for finer threads, including “Dacron” for “Dacron” fabrics, organdy, “Dacron,” marquisette, dotted Swiss, lawn, batiste and rayon lend themselves beautifully to the use of sewing machine attachments for ruffling, tucking, hemming, etc. Fiberglas stitches well and is best suited to straight panel type curtains with pleated headings. Use a mercerized thread and size 14 machine needle for Fortisan, synthetics and the many blends.

The average machine stitch length for these fabrics should be about 12 stitches to the inch and the tensions easy enough to prevent puckering the fabrics, particularly sheer fabrics, such as batiste, nylons, ninons and soft rayon blends.

For Damask, brocades, taffetas, satins, etc., use silk or mercerized thread, size 14 or 11 needles of 12 to 14 stitches per inch.

Heavy weight fabrics, namely, linens, cotton Damasks, sailcloth, ticking, denims, etc., require a heavy-duty thread, a size 16 needle and a 12 stitch length.

For light or medium weight fabrics comparable to polished cottons, Chintz, linens, Glosheen, percale, antique satin and faille, use a mercerized thread, a size 14 needle and a 12 or 14 stitch length.

10

RETURN
RETURN
FIXTURE
WIDTH
FLOOR LENGTH
FRAME
JAM
SASH
SILL
SILL LENGTH
APRON
APRON LENGTH
BASEBOARD
CLEAR RUG

11

## Window Measurements

Before taking measurements, there are several points that should be taken into consideration: Is the window in proportion to the room? Will it contribute properly to the effect you wish to achieve? Do you have the right rods for hanging the type of drapery selected?

When you are satisfied with the window, then it is time to consider the type of materials for draperies and decide on the type of rod required.

It is a good idea to make a sketch of the room, noting the placement of windows and arrangement of furniture. Also take the width and height measurement of each window. Then visit the curtain and drapery department to get an idea of the type of fixtures available. At the same time, obtain small samples of the fabrics suited to the type of drapery you have in mind. Examine them in the room where they are to be used. Are they the right texture? Are the colors lively enough? Will they create the desired effect?

Purchase and mount the rods for the draperies. Fixtures should be mounted so that draperies, when hung, will cover the window frame. Now you are ready to take measurements.

There are three correct lengths for draperies—to the sill—to the lower edge of the apron—or to the floor. Full length draperies should just clear the floor or be long enough to crush on the floor.

For length—Measure from the top of the rod down—to the sill—to the lower edge of apron—or to the floor.

For width—Measure from edge to edge of window frame or from outer edges of fixture brackets. To this measurement add the “return” at either end; that is, the length from curve of rod to the wall.

12

#### Estimating Yardage for Over-Curtains or Draperies

The type of heading, the width of lower hem and the type of drapery; that is, lined, unlined or interlined, must be considered when estimating the yardage required. The fullness of draperies averages about twice the width of the space to be covered.

A stiffening; such as a strip of crinoline or buckram is used at the top to support the pleats.

For Lined Draperies—To length measurement, add 1″ for heading, 4″ for hem and 3½″ for bottom hem.

Example—If length from top of rod is 90″, add 1″ plus 4″ plus 3½″. This equals 98½″ for one length, or 5½ yards for the two lengths.

For Unlined Draperies—To length measurement, add 1″ for heading, 4½″ for top hem and seam, and 3½″ for lower hem. A 4″ wide strip of crinoline is used at the top of both lined and unlined drapes.

If a double hem is used at the bottom, then add 6″ instead of 3½″ for hem in either lined or unlined drapes.

For Interlined Draperies—To length measurement, add 1″ for heading, 3″ for top hem and 3″ for bottom hem.

When using ready-made headings for pleats, add to the length measurement 1½″ for heading and seam, and 3½″ for bottom hem.

French Doors or Window

The rod should be placed so that the drapery, when hung, covers the glass portion of the window. Take measurement from top of upper rod to lower part of lower rod. To this measurement, add 2½″ at the top and 2½″ at the bottom. This allows for a 1½″ hem, top and bottom, plus ¼″ seam allowance. The 1½″ hem is for a ¾″ casing and ¾″ heading.

FIXTURE
FOR WIDTH
MEASURE FROM TOP AND BOTTOM OF FIXTURE
FIXTURE

13

#### Recessed Windows

When draperies are hung flush with the wall, measurements are taken inside the recess. A spring socket type of fixture is available for this type of window. Always measure from the top of the rod, except for Cafe curtains. Usually a ring, “sew-on” or “clip-on” type is used. In this case, measure from lower part of circle to lower part of next section, or to the sill. Add depth of top finish plus hem to this measurement.

Oval spring socket. Round spring socket.

#### Sliding Windows or Doors

Hook over or dual wheel design. Cord tension pulley. Install on wall, baseboard or floor.

These windows are usually treated as one. Draperies, in two sections, are hung on a pole or traverse rod and are drawn to the center, one section overlapping the other about 2″. Take length measurement from top of rod to the floor. To this measurement, add 5½″ for heading and top hem and 3½″ for bottom hem. If double hems are used, add 9″ at the top plus 6″ for bottom hem. To the width, add 3″ at either end for return of curtain from fixture to wall.

Two-way traverse rod.

#### Projected Window

To permit ease when opening or closing the window, the fixture should extend a little beyond the window on either side. Use a simple fixture, an oval or round rod, and a draw type of drapery. If drapery is to be shirred on the rod, take measurement from top of rod to lower edge of window. To length measurement, add 2½″ for a 1½″ hem which forms the casing and heading, and 2¾″ to 2½″ bottom hem. If sew-on or clip-on rings are used, measure from lower circle of ring to edge of window. To this measurement, add depth of top and bottom hem.

14

#### Awning Window

The type of drapery determines points of measurement. With tier type draperies, one for each section of the window, the measurements are taken from top to bottom of each section. Draperies hung from the top extending to lower edge of window or floor are measured from top of fixture for length desired. Tier type or cafe sections should be long enough to overlap the heading of the section below. Follow same procedure for measuring as for projected window. These draperies should be full—1½ times the width for medium weight fabrics, such as Chintz, Glosheen, etc., to three times the width when using sheer fabrics.

#### Methods of installing

Curtain and drapery rods, brackets and valance boards should be mounted securely to the wall to support heavy draperies. This can be a problem unless you use the right screws or bolts. There is a correct screw and bolt available for every type of wall—brick, concrete or plaster walls.

PLASTER SCREW—For plaster or dry walls.

PLASTIC PLUG—Use in brick wall for plug, then insert screw.

MOLLY BOLT—Use in plaster, brick or concrete wall.

TOGGLE BOLT—Use in frame or plaster walls where there is a separation between outer and inner walls.

15

## Construction Details

Draperies or over curtains are made of medium weight or heavy fabrics. They may be unlined, lined or lined and interlined, depending on the fabric and its treatment—whether formal or informal.

There are three accepted lengths for draperies—to the window sill—to the bottom of the window apron—or to the floor. Floor length is most generally used, and for very formal treatments, the drapery is often made long enough to crush on the floor. Draperies hang straight from the rod to the floor. If they meet at the top center, they may be draped to either side and held with ornamental tie-backs or those made of the same material.

When the type and design of draperies have been decided upon and the right type of rods have been mounted, then measurements for draperies can be taken.

Measure from the top of the rod down for length desired. Then add to length measurement the allowance for top and bottom hems. Review chapter on “Fabrics” before cutting lengths for draperies.

16

#### Unlined Draperies

These draperies are informal in treatment and are usually made of light or medium weight fabrics. Most any type of top finish, shirring or pleats is suitable. A plain valance or cornice board may be used. For a pleated heading, allow 5½″ at the top for heading and 5½″ at the bottom for a 2½″ double hem. Cut strips of crinoline or lawn for stiffening 4″ wide and 3″ shorter than the width of each drapery length. Pin strip to underside of heading ½″ from the top, starting 1½″ from the edge. Stitch along lower edge of strip, then turn top edge of fabric over stiffening ½″ and stitch. Turn top hem to underside along edge of stiffening. Press and pin in place.

Side hems may be put in by hand, machine stitched or blind stitched. For hand stitching or straight machine stitching, turn edge ½″ to underside; then turn 1″ for hem. Pin hem in place for stitching.

To blind-stitch hem, using the Zigzag Sewing Machine or the Zigzag Attachment, pin hem in place; then run a row of hand basting ¼″ from turned edge. With wrong side of drapery up, turn hem under to right side, exposing the ¼″ edge. Turn 2½″ double hem at the bottom and finish by hand or machine stitch.

Stitch stiffening to top of drapery.

STIFFENING
1½″ BOTH SIDES FOR HEMS
UNDERSIDE OF MATERIAL

Finish side hem by hand, using slip-stitch.

17

Side hem basted for blind-stitch hemming.

Blind-stitch hemming, using the Zigzag Sewing Machine.

Double hems with corners cut out to relieve bulk.

Finishing double side hems and bottom hem by hand.

18

If 1″ double side hems are used, cut stiffening 4″ shorter than the width of each drapery length. When using a heading with woven-in pockets for pleater pins, (available by the yard) allow 2″ at the top for heading and seam. Pin right side of heading to right side of drapery ⁵/₁₆″ below edge across the top. Consider the ″return″ of the drapery at each side, and position woven-in pockets so that the pleat comes at the turn of the rod. Stitch, taking ½″ seam; then turn heading to underside. Press and stitch ¼″ from the lower edge of the heading.

Type of hook used for forming pleats and hanging draperies.

RIGHT SIDE OF MATERIAL
Place pleat tape at top, ⁵/₁₆″ from edge. Stitch ½″ from edge.

1½″ BOTH SIDES FOR HEM
WRONG SIDE OF PLEAT TAPE

Tape turned to underside. Stitch tape to drapery at lower edge. Machine stitch 1″ side hems.

SLOTTED SIDE OF PLEAT TAPE

19

#### Lined Draperies

Lining in proportion to drapery length.

2″
TOP 4″ HEM
7″
LINING
3″
2″

Draperies are lined for the protection of the fabric. Linings also give weight to the draperies, causing them to hang in deeper folds. A sun-fast white, soft gray or cream colored sateen is generally used as the lining fabric.

Linings, just as drapery fabrics, must be cut straight with the crosswise and lengthwise grains.

Always start with a straight crosswise edge. This is obtained by drawing a crosswise thread and cutting on drawn thread. If fabric slopes up on one edge, then it should be straightened before pieces are cut.

Very often, when fabrics are rolled on the boards at the mills, the fabric is rolled more tightly on one end than at the other, drawing the crosswise threads (weft) in a diagonal line. This is apt to be true in loosely woven fabrics and particularly lining fabric.

To straighten fabric, first remove selvages, pull fabric gently but effectively, stretching it diagonally from corner to corner; then alternate. Grasp the fabric so that you will neither injure nor wrinkle it. Press before seaming.

Lining should be cut to allow for a 2″ hem at the bottom and a ½″ seam across the top and sides.

Illustration is for a drapery 2½ yards long, finished with 4″ top hem, 1″ side hems and 3″ bottom hem. Drapery length would measure 20 98½″ and lining length, 88½″. The average hem widths, 3″ and 4″, were used in figuring measurements. The width of hems vary. There is no fixed rule. They may be 3″—4″—5″ or even 7″ at the top and 2″—2½″—3″ or 4″ at the bottom. In many cases the bottom hem is doubled, particularly in sheer or lightweight fabrics. Also the center side hem may be as much as 2″ wide and the outer hem 1″. In this case, the lining is cut 6″ narrower than the drapery. Before taking measurements for draperies, review section on Window Measurements.

To join lining, turn top edge of lining to underside ½″ and press. Pin lining and drapery together, starting 7½″ from the top. Stitch from top of lining down to 4½″ of lower edge of lining, taking a ½″ seam. Back-stitch at the beginning and end of seam. Press seam as stitched; then clip seam every 3″ or 4″. Press the seam open. Pin, from hem to hem, a 4″ wide strip of stiffening to underside across the top. Stitch and press.

Straightening material—Pull diagonally from low corner.

Joining lining to drapery.

RIGHT SIDE OF MATERIAL
7½″
LINING

Stiffening stitched to heading.

STIFFENING
1½″ FOR HEM BOTH SIDES
UNDERSIDE OF MATERIAL

Turn drapery right side out and adjust hems on either side. Be sure seams are spread open. Press and pin. Turn top hem to underside. Pin and press. Turn and miter side 21 hem. Cut out top hem even with stiffening and within 1″ of the top. Pin lining to hem, overlapping lower edge ½″. Side hem and mitered corner above the lining should be slip-stitched by hand; then slip-stitch lining to top hem. Press. Allow draperies to hang for 2 or 3 days before putting in lower hems. Then adjust length of drapery so that it clears the rug or floor. Turn edge under ½″; then turn hem width. If an allowance is made for a double hem, first turn to underside one-half the width allowed, then turn again the same width, enclosing first turn. Slip-stitch hem by hand or stitch by machine. The lining hem overlaps the drapery hem approximately 1″. Allowance is made for a 2″ hem with ½″ for seam. The lining hem hangs free of the curtain and is held in position with french tacks spaced about 12″ apart. To french tack, take 3 or 4 stitches first at top of drapery hem, then lining hem, then drapery hem, etc., leaving a ½″ or ¾″ length between. Blanket stitch over the full length of these strands of thread. Fasten thread at end of tack. Draperies should be anchored at top of return and lower side hems.

Use a sew-on or pin-on weight at bottom of center hems.

(See illustration at top of page 22.)

Cut out end of top hem to eliminate bulk.

LINING TURNED BACK

Lining slip-stitched to top hem.

LINING

Making a French tack.

LINING

22

‘Sew-on’ or ‘pin-on’ weights.

Lined drapery with pleater tape heading.

Side hems tacked to insure evenness.

When using a tape with woven-in pockets for pleater pins, allow 2″ above the rod for heading and seam. See instructions under the section Unlined Draperies for joining tape to heading. Join lining; then clip and press seams. Turn drapery to right side and pin lining to bottom of tape, overlapping ¼″. Stitch and press; then finish side hems above lining by hand.

It is a good idea to tack the side hems along stitching line. This prevents them from slipping and hems always appear sharper. Using matching thread and working from the underside, insert needle through the seam down through to the right side, picking up a thread or two of the fabric. Then bring needle back up through the seam. Insert needle at the same point and direct needle along the seam between the hem a distance of 1″. Bring needle up through seam; then direct needle down through seam at same point, picking up two or three threads, and then up through seam again. Continue this tacking the length of the hem.

#### Drapery lined to top

There are times that draperies are lined to the top instead of using a hem, particularly when a valance or cornice board is used. To the length 23 measurement, add 1½″ at the top for heading and seam. Cut lining in proportion. Stitch lining and drapery lengths together, bringing edges even at the top. Clip seam and press open. Cut stiffening the length of drapery width. Pin and stitch stiffening across the top, taking ½″ seam. Turn drapery right side out, enclosing heading. Press top and side hems. Finish hems at the bottom the same as for lined draperies.

Joining stiffening to lining and drapery at top.

Drapery turned to right side.

#### Interlined Draperies

Draperies are often interlined, particularly in very formal rooms, or when the character of the material is such that the extra weight is necessary for its protection. Interlining also adds to the draping quality and elegance of the fabric.

For an interlining fabric, use good quality cotton flannel. Cut interlining the exact measurements of draperies when finished; that is, if draperies have 1½″ hems on each side and 3″ hems, top and bottom, then cut interlining 3″ narrower and 6″ shorter than drapery fabric. Spread material right side down.

Tack interlining to drapery at center and between center and side hems.

3″
TACK DOWN THROUGH CENTER
INTERLINING FOLDED LENGTHWISE FOR TACKING
1½″

24

Turn and baste hems—side, top, and bottom.

UNDERSIDE OF MATERIAL
INTERLINING

Fold interlining through lengthwise center. Place fold on exact center of drapery fabric and tack together loosely. Take a stitch in the drapery; bring needle up through fold of interlining and leave a loop. Space about 6″; take a stitch in drapery, then interlining, then drapery, etc. Do not pull thread taut. When row is finished, fold interlining halfway between center and edge on both sides and tack in the same manner, making three rows of vertical tacking.

Catch-stitch hems to interlining.

Turn side hems back over interlining. Pin and baste. Then turn top and bottom hems. Pin and baste. Miter hems at corners. All hems may be catch-stitched to the interlining, and the lining slip-stitched to top and side hems. Linings may also be joined by machine. Turn hem and baste; then pin lining to drapery and stitch, taking ½″ seam. Press seam as stitched. Then clip and press seam open the same as for all lined curtains and draperies.

25

Turn sides and top of lining under ½″. Pin in place, slip-stitch.

When lining is joined to drapery by machine, tack interlining and lining together along seam. Take stitch in seam, then in interlining. Space stitching 3″ or 4″ apart. Do not draw thread taut. Turn top and bottom hems and catch-stitch. Pin lining to hem across the top and slip-stitch. Turn hem in lining and stitch. Allowance should be made for a 2″ hem, overlapping the hem in drapery approximately 1″. Use french tacks between lining hem and drapery to hold lining in place. Use either ‘sew-on’ or ‘pin-on’ weight at bottom of side hems.

When lining is machine stitched to drapery, tack seam to interlining.

French tacks hold drapery and lining together.

26

## Measuring for Pleats

The use of pleats is one of the most effective ways of controlling the fullness of a drapery that is made to hang in balanced, graceful folds. The types most generally used are the pinch pleat, the French pleat, the box pleat and the cartridge pleat.

Pleats should be made in groups of uneven numbers, 5-7-9, or as many as are required to take up the amount allowed for fullness. For very sheer fabrics, the allowance for fullness should be 3 times the width of the window or space to be covered. To figure the spacings and amount to be taken up in pleats, take the measurement of the space to be covered plus the return; that is, the distance from turn of rod to the wall or the bracket supporting the rod on either end, plus the overlap at the center when curtains are drawn together. The width allowed for draperies minus these three measurements is to be taken up in pleats.

The fullness of each type of pleat and space between depends on the weight of the material and amount allowed for fullness of the curtain.

For Example: If one half of the width to be covered is 49″ then one section of the drapery would be about 144″ wide after finishing side hems. To width of window area (49″), add 3″ for return and 1″ for center overlap. This totals 53″. 144″ minus 53″ equals 91″ for pleats. Allowing 7″ for each pleat, 13 pleats will be required to take up the fullness.

Please Note—3″ for return is used as an example. The return can be 4″ or 5″, depending on type of rod or bracket. Always measure the return.

27

#### Steps to Pleats

Always measure and mark the exact position and width for all pleats and spacings before stitching.

Measure the width of the return from outer edge. Then measure for the first pleat at the curve of the rod. Place second pleat on opposite side 2″ from center edge. The third pleat is placed at the exact center between the first and second pleat. The remaining number of pleats required is evenly spaced between the 1st and 3rd and between the 2nd and 3rd pleats. To form pleats, bring markings for pleats together. Pin; then stitch from top to ¾″ below the heading, reversing the stitch at either end.

1. Bring the markings together for pleat and pin.

2. Stitch from top to about ¾″ below heading, reversing stitch at each end.

These steps are the same for all types of pleats.

Pinch Pleat—Divide the large pleat evenly into three smaller pleats; press in firmly and stitch across the three folds at lower edge of heading. The Pinch pleat is a favorite finish for most types of draperies and is particularly good when draperies are made of a heavier fabric.

28

French Pleat—At lower edge of heading, divide large pleat into three smaller pleats and run needle and thread through three pleats several times, drawing thread tight. Then fasten thread securely underneath.

Box Pleat—The large pleat is spread an equal distance on each side of stitching and pressed flat. Box pleats should be about 2″ wide, taking up 4″ fullness.

When figuring these pleats, try for uniformity; that is, the space between each pleat (from fold to fold) should be the same as the width of pleat. Box pleats should be about 2″ wide, taking up 4″ fullness.

Cartridge Pleat—This is a round pleat left loose and filled with cotton, Kapok or a roll of stiff paper. The pleats take up 2″ to 2½″ and are spaced from 2″ to 3″ apart for draw type draperies.

1. Type of pins used if curtain is hung from traverse rod.

2. Type of pins used if curtain is hung from rod with rings or from traverse rod mounted against ceiling.

29

#### Doors or Windows Opening Out

Box Pleats, extending above the heading to form a loop, make an interesting treatment for unlined curtains draping a French window or door that opens out.

Draperies hang from a rod drawn through the loops. Fabrics, such as Fortisan blends, antique satin, taffetas and sheer linens are suitable for these curtains.

Measure from top of rod to floor for length. Add 9½″ at top for seam, loops, and facing and 6″ for a 3″ double bottom hem. Allow 3 times the width of space to be covered for fullness.

Example: If space to be covered is 52″, 3 lengths of 48″ fabric are required. Cut one length through center and join each half width to each one of the full widths. Each section measures approximately 70″. 70″ minus 4″ for 1″ double hems and 3″ for return equals 63″. 7 pleats × 5″ = 35″. 63″ minus 35″ = 28″ for space to be covered and center overlap.

1. Measuring for pleats, spacings and loops. Pleats may be wider or as narrow as desired. Spacings may vary, depending on weight of material. Always consider the pleat overlap.

30

2. Turn top to right side 9½″. Use a stiffening or stay of lawn or organdy for most light and medium weight materials. Arrows indicate stitching lines.

3. Material is cut out between loops. Seams are slashed diagonally at corners to line of stitching. Press. If stiffening is not used as shown in sketches 1 and 2, stitch 4″ strip of crinoline to hem as shown above. This lends support to pleats.

31

4. Turn loops right side out and hem to underside. Press. Pin in pleat, stitch same as for Box pleat. Spread pleat, press.

5. Fasten loops to back of pleat by hand. Anchor curtains at side, top and bottom as shown page 15.

32

Pattern for tie-back pinned to material.

Tie-back stitched—Seam blended ready for turning.

#### Tie-Backs

Fabric tie-backs for draperies are usually tailored, straight or shaped bands which match or harmonize with the drapery in color and design. The fullness of the drapery determines the length of the tie-back. To estimate length, loop a strip of material around the drapery, drawing it back to side of window for the best effect. Lengths may vary from 18″ to 24″ and can be 2½″ or more in width. They are usually lined or faced and interlined. Use a stiffening of heavy muslin or crinoline in a shaped band. For shaped band, cut a paper pattern about 3″ or 4″ wide in the center, tapering to 2″ or 2½″ at the end as illustrated. Cut fabric, lining and stiffening the same as pattern, allowing for a ⅜″ seam on all edges.

Pin stiffening to underside of band, and lining to right side of material—right sides together. Stitch, leaving an opening of 3″ or 4″ for turning.

Trim stiffening to stitching line and blend edge of lining. Press. Turn band right side out and press. Slip-stitch lining to band at opening.

Sew small bone rings or very narrow fabric loops at ends of band. These loop over a hook fastened to side of window.

#### Anchoring Draperies

Outside edges of draperies should hang against the wall in a straight taut line. Sew a plastic ring to the bottom hem. Place a cup hook in the wall or the baseboard in line with the hem.

33

## Meet the sewing machine with tomorrow written all over it.

Does all 3 kinds of sewing—straight, zig-zag and chainstitch.
Hundreds of zig-zag patterns built-in—just touch a button and sew.
Spinning reel thread system—for smooth, even thread flow.
New speed switch—set your own sewing speed, fast or slow.
New built-in needle threader—ends that last little sewing worry.
Push-Button Bobbin—winds right in the machine.
Exclusive Slant Needle—see better, sew smoother.
New 4-position throat plate lever—an extra for delicate fabrics.
New buttonholer device—makes 7 kinds of buttonholes easily.

New Golden Touch & Sew[1] sewing machine by Singer. Be the girl with the golden touch on this newest and most fabulous of our growing family of Touch & Sew sewing machines with the Push-Button Bobbin. One of five new models starting at $149.95.

See SINGER COMPANY in phone book for Shop nearest you.

34

SINGER SEWING LIBRARY
You’re sure to want a complete set

Here are the newest, most informative, “how to” sewing books available today! Together they make up a complete dressmaking—home decorations library. Fully illustrated, each one covers its subject step-by-step, answering all your questions—in as few words as possible—almost before you ask them. Choose your needs from the selection of books listed below.

101—HOW TO MAKE CURTAINS
102—HOW TO MAKE DRAPERIES
103—HOW TO MAKE VALANCES
104—HOW TO MAKE BEDSPREADS
105—HOW TO LAY OUT A PATTERN AND CUT
106—HOW TO MEASURE, ALTER AND FIT
107—HOW TO MAKE SEAMS AND FINISHES
108—HOW TO MAKE SLEEVES
109—HOW TO MAKE BUTTONHOLES AND POCKETS
110—HOW TO MAKE COLLARS, FINISH NECKLINES
111—HOW TO MAKE ZIPPER CLOSURES
112—HOW TO MAKE BELTS AND HEMS
113—HOW TO MAKE SLIP COVERS
114—HOW TO MAKE CAFE CURTAINS
115—THINGS FOR LITTLE GIRLS TO SEW
116—CREATING CHARM WHEN SEWING FOR GIRLS
117—HOW TO REINFORCE, REPAIR AND REFIT
118—HOW TO DO DRESSMAKER TAILORING
119—HOW TO MAKE APRONS
120—HOW TO MAKE CUSHIONS, PILLOWS, AND BOLSTERS
121—HOW TO SEW FOR BABIES

Singer Sewing library Books are available at Singer Centers, variety, chain and department stores ... where you will also find the SINGER SEWING SHELF—for sewing machine parts and supplies.

[1]A Trademark of THE SINGER COMPANY

Cover Photograph reprinted from the BRIDE’S MAGAZINE
Copyright 1957, The Condé Nast Publications, Inc.

Printed in the United States of America Book No. 102

## Transcriber’s Notes

- Silently corrected a few typos.
- Retained publication information from the printed edition: this eBook is public-domain in the country of publication.
- In the text versions only, text in italics is delimited by _underscores_.

*** END OF THE PROJECT GUTENBERG EBOOK HOW TO MAKE DRAPERIES ***
Updated editions will replace the previous one—the old editions will be renamed.
Creating the works from print editions not protected by U.S. copyright law means that no one owns a United States copyright in these works, so the Foundation (and you!) can copy and distribute it in the United States without permission and without paying copyright royalties. Special rules, set forth in the General Terms of Use part of this license, apply to copying and distributing Project Gutenberg™ electronic works to protect the PROJECT GUTENBERG™ concept and trademark. Project Gutenberg is a registered trademark, and may not be used if you charge for an eBook, except by following the terms of the trademark license, including paying royalties for use of the Project Gutenberg trademark. If you do not charge anything for copies of this eBook, complying with the trademark license is very easy. You may use this eBook for nearly any purpose such as creation of derivative works, reports, performances and research. Project Gutenberg eBooks may be modified and printed and given away—you may do practically ANYTHING in the United States with eBooks not protected by U.S. copyright law. Redistribution is subject to the trademark license, especially commercial redistribution.
START: FULL LICENSE

## THE FULL PROJECT GUTENBERG™ LICENSE

PLEASE READ THIS BEFORE YOU DISTRIBUTE OR USE THIS WORK
To protect the Project Gutenberg™ mission of promoting the free distribution of electronic works, by using or distributing this work (or any other work associated in any way with the phrase “Project Gutenberg”), you agree to comply with all the terms of the Full Project Gutenberg License available with this file or online at www.gutenberg.org/license.
Section 1. General Terms of Use and Redistributing Project Gutenberg electronic works
1.A. By reading or using any part of this Project Gutenberg electronic work, you indicate that you have read, understand, agree to and accept all the terms of this license and intellectual property (trademark/copyright) agreement. If you do not agree to abide by all the terms of this agreement, you must cease using and return or destroy all copies of Project Gutenberg electronic works in your possession. If you paid a fee for obtaining a copy of or access to a Project Gutenberg electronic work and you do not agree to be bound by the terms of this agreement, you may obtain a refund from the person or entity to whom you paid the fee as set forth in paragraph 1.E.8.
1.B. “Project Gutenberg” is a registered trademark. It may only be used on or associated in any way with an electronic work by people who agree to be bound by the terms of this agreement. There are a few things that you can do with most Project Gutenberg electronic works even without complying with the full terms of this agreement. See paragraph 1.C below. There are a lot of things you can do with Project Gutenberg electronic works if you follow the terms of this agreement and help preserve free future access to Project Gutenberg electronic works. See paragraph 1.E below.
1.C. The Project Gutenberg Literary Archive Foundation (“the Foundation” or PGLAF), owns a compilation copyright in the collection of Project Gutenberg electronic works. Nearly all the individual works in the collection are in the public domain in the United States. If an individual work is unprotected by copyright law in the United States and you are located in the United States, we do not claim a right to prevent you from copying, distributing, performing, displaying or creating derivative works based on the work as long as all references to Project Gutenberg are removed. Of course, we hope that you will support the Project Gutenberg mission of promoting free access to electronic works by freely sharing Project Gutenberg works in compliance with the terms of this agreement for keeping the Project Gutenberg name associated with the work. You can easily comply with the terms of this agreement by keeping this work in the same format with its attached full Project Gutenberg License when you share it without charge with others.
1.D. The copyright laws of the place where you are located also govern what you can do with this work. Copyright laws in most countries are in a constant state of change. If you are outside the United States, check the laws of your country in addition to the terms of this agreement before downloading, copying, displaying, performing, distributing or creating derivative works based on this work or any other Project Gutenberg work. The Foundation makes no representations concerning the copyright status of any work in any country other than the United States.
1.E. Unless you have removed all references to Project Gutenberg:
1.E.1. The following sentence, with active links to, or other immediate access to, the full Project Gutenberg License must appear prominently whenever any copy of a Project Gutenberg work (any work on which the phrase “Project Gutenberg” appears, or with which the phrase “Project Gutenberg” is associated) is accessed, displayed, performed, viewed, copied or distributed:

> This eBook is for the use of anyone anywhere in the United States and most other parts of the world at no cost and with almost no restrictions whatsoever. You may copy it, give it away or re-use it under the terms of the Project Gutenberg™ License included with this eBook or online at www.gutenberg.org. If you are not located in the United States, you will have to check the laws of the country where you are located before using this eBook.

1.E.2. If an individual Project Gutenberg electronic work is derived from texts not protected by U.S. copyright law (does not contain a notice indicating that it is posted with permission of the copyright holder), the work can be copied and distributed to anyone in the United States without paying any fees or charges. If you are redistributing or providing access to a work with the phrase “Project Gutenberg” associated with or appearing on the work, you must comply either with the requirements of paragraphs 1.E.1 through 1.E.7 or obtain permission for the use of the work and the Project Gutenberg trademark as set forth in paragraphs 1.E.8 or 1.E.9.
1.E.3. If an individual Project Gutenberg electronic work is posted with the permission of the copyright holder, your use and distribution must comply with both paragraphs 1.E.1 through 1.E.7 and any additional terms imposed by the copyright holder. Additional terms will be linked to the Project Gutenberg License for all works posted with the permission of the copyright holder found at the beginning of this work.
1.E.4. Do not unlink or detach or remove the full Project Gutenberg License terms from this work, or any files containing a part of this work or any other work associated with Project Gutenberg.
1.E.5. Do not copy, display, perform, distribute or redistribute this electronic work, or any part of this electronic work, without prominently displaying the sentence set forth in paragraph 1.E.1 with active links or immediate access to the full terms of the Project Gutenberg License.
1.E.6. You may convert to and distribute this work in any binary, compressed, marked up, nonproprietary or proprietary form, including any word processing or hypertext form. However, if you provide access to or distribute copies of a Project Gutenberg work in a format other than “Plain Vanilla ASCII” or other format used in the official version posted on the official Project Gutenberg website (www.gutenberg.org), you must, at no additional cost, fee or expense to the user, provide a copy, a means of exporting a copy, or a means of obtaining a copy upon request, of the work in its original “Plain Vanilla ASCII” or other form. Any alternate format must include the full Project Gutenberg License as specified in paragraph 1.E.1.
1.E.7. Do not charge a fee for access to, viewing, displaying, performing, copying or distributing any Project Gutenberg works unless you comply with paragraph 1.E.8 or 1.E.9.
1.E.8. You may charge a reasonable fee for copies of or providing access to or distributing Project Gutenberg electronic works provided that:

- • You pay a royalty fee of 20% of the gross profits you derive from the use of Project Gutenberg works calculated using the method you already use to calculate your applicable taxes. The fee is owed to the owner of the Project Gutenberg trademark, but he has agreed to donate royalties under this paragraph to the Project Gutenberg Literary Archive Foundation. Royalty payments must be paid within 60 days following each date on which you prepare (or are legally required to prepare) your periodic tax returns. Royalty payments should be clearly marked as such and sent to the Project Gutenberg Literary Archive Foundation at the address specified in Section 4, “Information about donations to the Project Gutenberg Literary Archive Foundation.”
- • You provide a full refund of any money paid by a user who notifies you in writing (or by e-mail) within 30 days of receipt that s/he does not agree to the terms of the full Project Gutenberg™ License. You must require such a user to return or destroy all copies of the works possessed in a physical medium and discontinue all use of and all access to other copies of Project Gutenberg™ works.
- • You provide, in accordance with paragraph 1.F.3, a full refund of any money paid for a work or a replacement copy, if a defect in the electronic work is discovered and reported to you within 90 days of receipt of the work.
- • You comply with all other terms of this agreement for free distribution of Project Gutenberg™ works.

1.E.9. If you wish to charge a fee or distribute a Project Gutenberg™ electronic work or group of works on different terms than are set forth in this agreement, you must obtain permission in writing from the Project Gutenberg Literary Archive Foundation, the manager of the Project Gutenberg™ trademark. Contact the Foundation as set forth in Section 3 below.
1.F.
1.F.1. Project Gutenberg volunteers and employees expend considerable effort to identify, do copyright research on, transcribe and proofread works not protected by U.S. copyright law in creating the Project Gutenberg™ collection. Despite these efforts, Project Gutenberg™ electronic works, and the medium on which they may be stored, may contain “Defects,” such as, but not limited to, incomplete, inaccurate or corrupt data, transcription errors, a copyright or other intellectual property infringement, a defective or damaged disk or other medium, a computer virus, or computer codes that damage or cannot be read by your equipment.
1.F.2. LIMITED WARRANTY, DISCLAIMER OF DAMAGES - Except for the “Right of Replacement or Refund” described in paragraph 1.F.3, the Project Gutenberg Literary Archive Foundation, the owner of the Project Gutenberg™ trademark, and any other party distributing a Project Gutenberg™ electronic work under this agreement, disclaim all liability to you for damages, costs and expenses, including legal fees. YOU AGREE THAT YOU HAVE NO REMEDIES FOR NEGLIGENCE, STRICT LIABILITY, BREACH OF WARRANTY OR BREACH OF CONTRACT EXCEPT THOSE PROVIDED IN PARAGRAPH 1.F.3. YOU AGREE THAT THE FOUNDATION, THE TRADEMARK OWNER, AND ANY DISTRIBUTOR UNDER THIS AGREEMENT WILL NOT BE LIABLE TO YOU FOR ACTUAL, DIRECT, INDIRECT, CONSEQUENTIAL, PUNITIVE OR INCIDENTAL DAMAGES EVEN IF YOU GIVE NOTICE OF THE POSSIBILITY OF SUCH DAMAGE.
1.F.3. LIMITED RIGHT OF REPLACEMENT OR REFUND - If you discover a defect in this electronic work within 90 days of receiving it, you can receive a refund of the money (if any) you paid for it by sending a written explanation to the person you received the work from. If you received the work on a physical medium, you must return the medium with your written explanation. The person or entity that provided you with the defective work may elect to provide a replacement copy in lieu of a refund. If you received the work electronically, the person or entity providing it to you may choose to give you a second opportunity to receive the work electronically in lieu of a refund. If the second copy is also defective, you may demand a refund in writing without further opportunities to fix the problem.
1.F.4. Except for the limited right of replacement or refund set forth in paragraph 1.F.3, this work is provided to you ‘AS-IS’, WITH NO OTHER WARRANTIES OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO WARRANTIES OF MERCHANTABILITY OR FITNESS FOR ANY PURPOSE.
1.F.5. Some states do not allow disclaimers of certain implied warranties or the exclusion or limitation of certain types of damages. If any disclaimer or limitation set forth in this agreement violates the law of the state applicable to this agreement, the agreement shall be interpreted to make the maximum disclaimer or limitation permitted by the applicable state law. The invalidity or unenforceability of any provision of this agreement shall not void the remaining provisions.
1.F.6. INDEMNITY - You agree to indemnify and hold the Foundation, the trademark owner, any agent or employee of the Foundation, anyone providing copies of Project Gutenberg™ electronic works in accordance with this agreement, and any volunteers associated with the production, promotion and distribution of Project Gutenberg™ electronic works, harmless from all liability, costs and expenses, including legal fees, that arise directly or indirectly from any of the following which you do or cause to occur: (a) distribution of this or any Project Gutenberg work, (b) alteration, modification, or additions or deletions to any Project Gutenberg work, and (c) any Defect you cause.
Section 2. Information about the Mission of Project Gutenberg
Project Gutenberg is synonymous with the free distribution of electronic works in formats readable by the widest variety of computers including obsolete, old, middle-aged and new computers. It exists because of the efforts of hundreds of volunteers and donations from people in all walks of life.
Volunteers and financial support to provide volunteers with the assistance they need are critical to reaching Project Gutenberg’s goals and ensuring that the Project Gutenberg collection will remain freely available for generations to come. In 2001, the Project Gutenberg Literary Archive Foundation was created to provide a secure and permanent future for Project Gutenberg and future generations. To learn more about the Project Gutenberg Literary Archive Foundation and how your efforts and donations can help, see Sections 3 and 4 and the Foundation information page at www.gutenberg.org.
Section 3. Information about the Project Gutenberg Literary Archive Foundation
The Project Gutenberg Literary Archive Foundation is a non-profit 501(c)(3) educational corporation organized under the laws of the state of Mississippi and granted tax exempt status by the Internal Revenue Service. The Foundation’s EIN or federal tax identification number is 64-6221541. Contributions to the Project Gutenberg Literary Archive Foundation are tax deductible to the full extent permitted by U.S. federal laws and your state’s laws.
The Foundation’s business office is located at 41 Watchung Plaza #516, Montclair NJ 07042, USA, +1 (862) 621-9288. Email contact links and up to date contact information can be found at the Foundation’s website and official page at www.gutenberg.org/contact
Section 4. Information about Donations to the Project Gutenberg Literary Archive Foundation
Project Gutenberg™ depends upon and cannot survive without widespread public support and donations to carry out its mission of increasing the number of public domain and licensed works that can be freely distributed in machine-readable form accessible by the widest array of equipment including outdated equipment. Many small donations ($1 to $5,000) are particularly important to maintaining tax exempt status with the IRS.
The Foundation is committed to complying with the laws regulating charities and charitable donations in all 50 states of the United States. Compliance requirements are not uniform and it takes a considerable effort, much paperwork and many fees to meet and keep up with these requirements. We do not solicit donations in locations where we have not received written confirmation of compliance. To SEND DONATIONS or determine the status of compliance for any particular state visit www.gutenberg.org/donate.
While we cannot and do not solicit contributions from states where we have not met the solicitation requirements, we know of no prohibition against accepting unsolicited donations from donors in such states who approach us with offers to donate.
International donations are gratefully accepted, but we cannot make any statements concerning tax treatment of donations received from outside the United States. U.S. laws alone swamp our small staff.
Please check the Project Gutenberg web pages for current donation methods and addresses. Donations are accepted in a number of other ways including checks, online payments and credit card donations. To donate, please visit: www.gutenberg.org/donate.
Section 5. General Information About Project Gutenberg electronic works
Professor Michael S. Hart was the originator of the Project Gutenberg concept of a library of electronic works that could be freely shared with anyone. For forty years, he produced and distributed Project Gutenberg eBooks with only a loose network of volunteer support.
Project Gutenberg eBooks are often created from several printed editions, all of which are confirmed as not protected by copyright in the U.S. unless a copyright notice is included. Thus, we do not necessarily keep eBooks in compliance with any particular paper edition.
Most people start at our website which has the main PG search facility: www.gutenberg.org.
This website includes information about Project Gutenberg, including how to make donations to the Project Gutenberg Literary Archive Foundation, how to help produce our new eBooks, and how to subscribe to our email newsletter to hear about new eBooks.